{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["倍特力"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"倍特力","index":0,"n_rows":14,"n_cols":8,"rows_kept":14,"merged":[[0,0,5,7],[13,1,13,5]],"flags":["formulas_cached_only"]}
["郊尾镇伍狮村IP数字广播系统项目"]
[]
[]
[]
[]
[]
["序号","名称","技术参数","单位","数量","单价（元）","金额（元）","备注"]
[1,"IP网络寻呼播控话筒","1、安装在主控室、值班室或领导办公室，可进行单向广播（对点、分区或全区）、双向对讲和监听。2、工业级3.4寸LCD显示屏，19个工业级金属按键，超强抗干扰性能，避免红外操作的不稳定因素；3、采用嵌入式计算机技术和DSP音频处理技术设计；采用高速工业级芯片，启动时间小于1秒钟；4、 内置1路网络硬件音频解码模块，支持TCP/IP、UDP、IGMP(组播)协议，实现网络化传输16位立体声CD音质的音频信号；5、内置2W全频高保真扬声器，实现双向通话和网络监听；6、 内置高性能DSP音效处理，支持数字回音消除、音频压缩功能；7、内置免提通话功能，支持自定义接听方式，支持耳麦；8、支持远程点播功能，支持1000级自定义音频优先级默音控制(支持多路信号放大、混音、三级优先控制、音调调节）；9、支持DHCP，兼容路由器、交换机、网桥网关、Modem、Intelnet、2G、3G、4G、组播、单播等任意网络结构；10、支持至少3种高安全的授权IP配置方案，安全系数远高于Web等远程配置方案；11、授权操作管理功能，支持服务器统一配置管理用户及密码；12、仿iOS平铺式菜单管理，消灭复杂的二级菜单；13、支持数字音频时光流逝的断点播放功能，确保广播同步效果；14、支持新配置注册智能语音提示功能；15、支持15KVESD保护，内置网络隔离防雷处理电路；16、1路PC机下载IP地址串口，用于修改网络解码模块IP地址；","台",1]
[2,"分控电脑","操作系统：DOS；主板芯片组：Intel H81；CPU系列：英特尔 酷睿i5 4代系列；最高睿频3600MHz；缓存：6MB；核心架构：Haswell；内存类型：DDR3 1600MHz；","台",1]
[3,"合并式防水音箱带功放","1.输出额定功率:60W/8Ω；2.网络接口：标准RJ45输入；3.支持协议：TCP/IP、UDP、IGMP(组播)；4.音频格式：MP3；5.采样率：8K-48KHz；6.传输速率：100Mbps；7.音频模式：16位CD音质；8.输出频率：80Hz~16KHz；9.谐波失真：≤1%；10.信噪比：>70dB；11.防水等级：IP54 ；12.输入电源：~220V 50Hz；13.喇叭单元：4”×4；14.功耗：≤70W","台","5"]
[4,"六类网络线","8*0.5无氧铜","米","500"]
[5,"电源线缆","2*1.0无氧铜","米","500"]
[6,"PVC电气管","6分管","米","500"]
[26,"合计"]